The wide variety of new Kuba 3 cable guides provide you with a range of different combination options. The two exterior joints hold the cable guide securely in the defined direction of movement. 
The cable guide can be fully customized to meet your personal needs and wishes. The area with the openings for the cables defines the front and exterior of the KUBA 3; data cables and electrical cables are fed through here into the cable guide. 
This system can be used to create a defined sequence of movement. To that end, we offer five different cable guide elements that each have different functions. 
Please note that the function described is transferred to the cable guide element below it in each case. The various cable guide elements are displayed in different colours in this brochure (see image: “Different types of cable guide elements”). 
Cable guide element FREE (item no. C-03011-0019204) - no pins on the underside of the cable guide element - it can move freely. 
Cable guide element FIXED (item no. C-03011-0019202) with wide pin on the underside. For all applications that require a fixed connection between the cable guide elements. 
Cable guide element FIXED with spacer (item no. C-03011-0019201) and wide pin on the underside. For all applications that require a chain of rigidly connected cable guide elements with magnetic holders, such as for use on the leg of a table or desk. The gap on the back of the magnetic holder, which is inherent in its design, is bridged by the spacer. 
Cable guide element INWARD (item no. C-03011-0019203) - the pins on the underside of the cable guide element point inward. The cable guide element can be moved from a straight position inward, but not outward.
Cable guide element OUTWARD (item no. C-03011-0019200) - the pins on the underside of the cable guide element point outward. The cable guide element can be moved from a straight position outward, but not inward. 
Ø 70 mm round tube adapter (item no. C-03011-0019211) - is used in connection with a magnetic element for attachment to a Ø 70 mm round tube. It should be mounted above a magnetic element. The cable guide element above it must be a fixed/rigid element (see image). 
Magnetic holder in chain - fixed (item no. C-03011-0019206) - the pins on the underside of the magnetic holder FIXED are wide and point downward - it is locked. The back has a built-in magnet with a nominal adhesive force of 19 kg. Additionally, the element includes 2 transparent elastic buffers for attachment to the table frame (see image). 
Magnet holder end of chain (item no. C-03011-0019205) - forms the lower end of the cable guide on the table leg. On the open front, the magnet holder holds the cables in the cable guide. The back has a built-in magnet with a nominal adhesive force of 19 kg. In addition, the element is provided with 2 non-slip elastic buffers. 
Adapter for metal base plate (item no. C-03011-0019209) allows the cable guide to be attached to the metal base plate C-03010-0029991. It snaps onto the base plate. 
What makes KUBA 3 special is the cable guide elements can only be moved in the pre-defined direction. The two exterior pivot points in combination with different types of cable guide elements mean that the cable guide can only move in the pre-defined direction or remain completely rigid.
